**HEALTHY HEADWATERS LAB**

**STANDARD OPERATING PROCEDURE**

|  |  |
| --- | --- |
| **Name** | Garmin etrex 10 – Mark Waypoint |
| **Version** | 1 |
| **Date** | 14/01/2020 |
| **Prepared by** | Lauren Weller |

1. Switch on the GPS (power button is located on the right-hand side and is marked with power symbol).
2. Use the mouse to scroll down to and select the “Satellite” section.
3. Wait for confirmation that the GPS has locked on/found satellites.
4. Return to the main menu.
5. Scroll up and select “Mark Waypoint”
6. Change the waypoint name (the GPS will autogenerate a number – you can click on this to change it alternatively record the waypoint number).
7. Add any notes as required.
8. Select Done to Mark the Waypoint.

General Tips:

* Ensure that a spare set of batteries is included when you take the GPS out as the battery life is short and there is little warning when the batteries are low before it dies.
* Compare the Waypoint location with the location of the University or your previous waypoint if you are unsure it is recording the waypoints correctly. You can also check the map view to see if you are in approximately the right area.

The university’s coordinates are N 42.30763 W 083.07292 for reference.